----------
Connect to: (2017/07/15 22:46:39)
hostname=hk500047.ftp.aliwebs.com
username=
startdir=
hk500047.ftp.aliwebs.com=47.52.1.58
220 Welcome to FTP service.
USER hk500047
331 Please specify the password.
PASS ***********
230 Login successful.
SYST
215 UNIX Type: L8
FEAT
211-Features:
 AUTH TLS
 EPRT
 EPSV
 MDTM
 PASV
 PBSZ
 PROT
 REST STREAM
 SIZE
 TVFS
 UTF8
211 End
HELP SITE
214-The following commands are recognized.
 ABOR ACCT ALLO APPE CDUP CWD  DELE EPRT EPSV FEAT HELP LIST MDTM MKD
 MODE NLST NOOP OPTS PASS PASV PORT PWD  QUIT REIN REST RETR RMD  RNFR
 RNTO SITE SIZE SMNT STAT STOR STOU STRU SYST TYPE USER XCUP XCWD XMKD
 XPWD XRMD
214 Help OK.
OPTS UTF8 ON
200 Always in UTF8 mode.
Connect ok!
PWD
257 "/" is the current directory
读取文件夹
TYPE A
200 Switching to ASCII mode.
PASV
227 Entering Passive Mode (47,52,1,58,234,101).
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
CWD myfolder
250 Directory successfully changed.
PWD
257 "/myfolder" is the current directory
读取文件夹
PASV
227 Entering Passive Mode (47,52,1,58,234,114).
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
CDUP
250 Directory successfully changed.
PWD
257 "/" is the current directory
TYPE I
200 Switching to Binary mode.
PASV
227 Entering Passive Mode (47,52,1,58,234,101).
RETR README
150 Opening BINARY mode data connection for README (745 bytes).
下载
等待服务器回应...
226 Transfer complete.
Copied (2017/07/15 22:47:01): ftp://hk500047.ftp.aliwebs.com//README -> C:\Users\phuslu\AppData\Local\Temp\_tc\README 745 字节, 22 KB/秒
CWD htdocs
250 Directory successfully changed.
PWD
257 "/htdocs" is the current directory
读取文件夹
TYPE A
200 Switching to ASCII mode.
PASV
227 Entering Passive Mode (47,52,1,58,234,96).
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
CWD ewh_logreport_no_delete
250 Directory successfully changed.
PWD
257 "/htdocs/ewh_logreport_no_delete" is the current directory
读取文件夹
PASV
227 Entering Passive Mode (47,52,1,58,234,114).
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
CDUP
250 Directory successfully changed.
PWD
257 "/htdocs" is the current directory
DELE default.html
250 Delete operation successful.
Deleted (2017/07/15 22:47:23): ftp://hk500047.ftp.aliwebs.com/htdocs/default.html
读取文件夹
PASV
227 Entering Passive Mode (47,52,1,58,234,100).
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
TYPE I
200 Switching to Binary mode.
PASV
227 Entering Passive Mode (47,52,1,58,234,98).
STOR index.php
150 Ok to send data.
上传
226 Transfer complete.
SIZE index.php
213 29505
Copied (2017/07/15 22:48:18): D:\index.php -> ftp://hk500047.ftp.aliwebs.com/htdocs/index.php 29,505 字节, 47 KB/秒
读取文件夹
TYPE A
200 Switching to ASCII mode.
PASV
227 Entering Passive Mode (47,52,1,58,234,101).
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
TYPE I
200 Switching to Binary mode.
PASV
227 Entering Passive Mode (47,52,1,58,234,96).
STOR fetch.php
150 Ok to send data.
上传
226 Transfer complete.
SIZE fetch.php
213 7303
Copied (2017/07/15 22:52:30): C:\Users\phuslu\Desktop\fetch.php -> ftp://hk500047.ftp.aliwebs.com/htdocs/fetch.php 7,303 字节, 41 KB/秒
读取文件夹
TYPE A
200 Switching to ASCII mode.
PASV
227 Entering Passive Mode (47,52,1,58,234,112).
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
QUIT
OFFLINE2, error=10054
----------
Connect to: (2017/09/27 23:28:02)
hostname=hk500047.ftp.aliwebs.com
username=hk500047
startdir=
hk500047.ftp.aliwebs.com=47.52.1.58
220 Welcome to FTP service.
USER hk500047
331 Please specify the password.
PASS ***********
230 Login successful.
SYST
215 UNIX Type: L8
FEAT
211-Features:
 AUTH TLS
 EPRT
 EPSV
 MDTM
 PASV
 PBSZ
 PROT
 REST STREAM
 SIZE
 TVFS
 UTF8
211 End
HELP SITE
214-The following commands are recognized.
 ABOR ACCT ALLO APPE CDUP CWD  DELE EPRT EPSV FEAT HELP LIST MDTM MKD
 MODE NLST NOOP OPTS PASS PASV PORT PWD  QUIT REIN REST RETR RMD  RNFR
 RNTO SITE SIZE SMNT STAT STOR STOU STRU SYST TYPE USER XCUP XCWD XMKD
 XPWD XRMD
214 Help OK.
OPTS UTF8 ON
200 Always in UTF8 mode.
Connect ok!
PWD
257 "/" is the current directory
读取文件夹
TYPE A
200 Switching to ASCII mode.
PASV
227 Entering Passive Mode (47,52,1,58,234,110).
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
CWD myfolder
250 Directory successfully changed.
PWD
257 "/myfolder" is the current directory
读取文件夹
PASV
227 Entering Passive Mode (47,52,1,58,234,111).
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
CDUP
250 Directory successfully changed.
PWD
257 "/" is the current directory
CWD htdocs
250 Directory successfully changed.
PWD
257 "/htdocs" is the current directory
读取文件夹
PASV
227 Entering Passive Mode (47,52,1,58,234,113).
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
TYPE I
200 Switching to Binary mode.
PASV
227 Entering Passive Mode (47,52,1,58,234,105).
STOR index.php
150 Ok to send data.
上传
226 Transfer complete.
SIZE index.php
213 25204
Copied (2017/09/27 23:28:15): C:\Users\phuslu\Desktop\index.php -> ftp://hk500047.ftp.aliwebs.com/htdocs/index.php 25,204 字节, 40 KB/秒
读取文件夹
TYPE A
200 Switching to ASCII mode.
PASV
227 Entering Passive Mode (47,52,1,58,234,107).
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
----------
Connect to: (08/26/2018 12:45:07)
hostname=192.168.2.2
username=anonymous
startdir=
220 pyftpdlib 1.5.1 ready.
USER anonymous
331 Username ok, send password.
PASS ***********
230 Login successful.
SYST
215 UNIX Type: L8
FEAT
211-Features supported:
 EPRT
 EPSV
 MDTM
 MLST type*;perm*;size*;modify*;unique*;unix.mode;unix.uid;unix.gid;
 REST STREAM
 SIZE
 TVFS
 UTF8
211 End FEAT.
HELP SITE
214 Syntax: SITE <SP> site-command (execute SITE command).
OPTS MLST type;perm;size;modify;unique;unix.mode;
200 MLST OPTS type;perm;size;modify;unique;unix.mode;
OPTS UTF8 ON
501 Invalid argument.
Connect ok!
PWD
257 "/" is the current directory.
读取文件夹
TYPE A
200 Type set to: ASCII.
PASV
227 Entering passive mode (192,168,2,2,223,71).
Server reports local IP -> Redirect to: 192.168.2.2
MLSD
125 Data connection already open. Transfer starting.
下载
等待服务器回应...
226 Transfer complete.
CWD .git
250 "/.git" is the current directory.
读取文件夹
PASV
227 Entering passive mode (192,168,2,2,8,107).
Server reports local IP -> Redirect to: 192.168.2.2
MLSD
125 Data connection already open. Transfer starting.
下载
等待服务器回应...
226 Transfer complete.
CWD branches
250 "/.git/branches" is the current directory.
读取文件夹
PASV
227 Entering passive mode (192,168,2,2,121,15).
Server reports local IP -> Redirect to: 192.168.2.2
MLSD
125 Data connection already open. Transfer starting.
下载
等待服务器回应...
226 Transfer complete.
CDUP
250 "/.git" is the current directory.
PWD
257 "/.git" is the current directory.
CDUP
250 "/" is the current directory.
PWD
257 "/" is the current directory.
TYPE I
200 Type set to: Binary.
PASV
227 Entering passive mode (192,168,2,2,243,167).
Server reports local IP -> Redirect to: 192.168.2.2
RETR promvps.error.log
125 Data connection already open. Transfer starting.
下载
等待服务器回应...
226 Transfer complete.
Copied (08/26/2018 12:45:24): ftp://192.168.2.2//promvps.error.log -> C:\Users\phuslu\AppData\Local\Temp\_tc\promvps.error.log 3,678 字节
PASV
227 Entering passive mode (192,168,2,2,211,123).
Server reports local IP -> Redirect to: 192.168.2.2
RETR promvps.error.log
125 Data connection already open. Transfer starting.
下载
等待服务器回应...
226 Transfer complete.
Copied (08/26/2018 12:45:26): ftp://192.168.2.2//promvps.error.log -> C:\Users\phuslu\AppData\Local\Temp\_tc\promvps.error.log 3,678 字节
DELE nohup.out
550 Not enough privileges.
QUIT
221 Goodbye.
----------
Connect to: (08/26/2018 12:46:03)
hostname=192.168.2.2
username=
startdir=
220 pyftpdlib 1.5.1 ready.
USER phuslu
331 Username ok, send password.
PASS ***********
530 Authentication failed.
QUIT
----------
Connect to: (08/30/2018 1:47:38)
hostname=lab.phus.lu
username=anonymous
startdir=
lab.phus.lu=153.3.130.136
220 (vsFTPd 3.0.3)
USER anonymous
331 Please specify the password.
PASS ***********
230 Login successful.
SYST
215 UNIX Type: L8
FEAT
211-Features:
 EPRT
 EPSV
 MDTM
 PASV
 REST STREAM
 SIZE
 TVFS
211 End
HELP SITE
214-The following commands are recognized.
 ABOR ACCT ALLO APPE CDUP CWD  DELE EPRT EPSV FEAT HELP LIST MDTM MKD
 MODE NLST NOOP OPTS PASS PASV PORT PWD  QUIT REIN REST RETR RMD  RNFR
 RNTO SITE SIZE SMNT STAT STOR STOU STRU SYST TYPE USER XCUP XCWD XMKD
 XPWD XRMD
214 Help OK.
OPTS UTF8 ON
200 Always in UTF8 mode.
Connect ok!
PWD
257 "/" is the current directory
读取文件夹
TYPE A
200 Switching to ASCII mode.
PASV
227 Entering Passive Mode (153,3,130,136,238,36).
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
CDUP
250 Directory successfully changed.
PWD
257 "/" is the current directory
----------
Connect to: (08/30/2018 1:48:50)
hostname=lab.phus.lu
username=anonymous
startdir=
lab.phus.lu=153.3.130.136
220 (vsFTPd 3.0.3)
USER anonymous
331 Please specify the password.
PASS ***********
230 Login successful.
SYST
215 UNIX Type: L8
FEAT
211-Features:
 EPRT
 EPSV
 MDTM
 PASV
 REST STREAM
 SIZE
 TVFS
211 End
HELP SITE
214-The following commands are recognized.
 ABOR ACCT ALLO APPE CDUP CWD  DELE EPRT EPSV FEAT HELP LIST MDTM MKD
 MODE NLST NOOP OPTS PASS PASV PORT PWD  QUIT REIN REST RETR RMD  RNFR
 RNTO SITE SIZE SMNT STAT STOR STOU STRU SYST TYPE USER XCUP XCWD XMKD
 XPWD XRMD
214 Help OK.
OPTS UTF8 ON
200 Always in UTF8 mode.
Connect ok!
PWD
257 "/" is the current directory
读取文件夹
TYPE A
200 Switching to ASCII mode.
PASV
227 Entering Passive Mode (153,3,130,136,164,159).
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
CDUP
250 Directory successfully changed.
PWD
257 "/" is the current directory
QUIT
221 Goodbye.
----------
Connect to: (08/30/2018 1:50:36)
hostname=lab.phus.lu
username=phuslu
startdir=/
lab.phus.lu=153.3.130.136
220 (vsFTPd 3.0.3)
USER phuslu
331 Please specify the password.
PASS ***********
230 Login successful.
SYST
215 UNIX Type: L8
FEAT
211-Features:
 EPRT
 EPSV
 MDTM
 PASV
 REST STREAM
 SIZE
 TVFS
211 End
HELP SITE
214-The following commands are recognized.
 ABOR ACCT ALLO APPE CDUP CWD  DELE EPRT EPSV FEAT HELP LIST MDTM MKD
 MODE NLST NOOP OPTS PASS PASV PORT PWD  QUIT REIN REST RETR RMD  RNFR
 RNTO SITE SIZE SMNT STAT STOR STOU STRU SYST TYPE USER XCUP XCWD XMKD
 XPWD XRMD
214 Help OK.
OPTS UTF8 ON
200 Always in UTF8 mode.
CWD /
250 Directory successfully changed.
Connect ok!
PWD
257 "/" is the current directory
读取文件夹
TYPE A
200 Switching to ASCII mode.
PASV
227 Entering Passive Mode (153,3,130,136,157,226).
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
CWD home
250 Directory successfully changed.
PWD
257 "/home" is the current directory
读取文件夹
PASV
227 Entering Passive Mode (153,3,130,136,59,150).
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
CWD download
250 Directory successfully changed.
PWD
257 "/home/download" is the current directory
读取文件夹
PASV
227 Entering Passive Mode (153,3,130,136,41,41).
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
CDUP
250 Directory successfully changed.
PWD
257 "/home" is the current directory
CWD h
250 Directory successfully changed.
PWD
257 "/home/h" is the current directory
读取文件夹
PASV
227 Entering Passive Mode (153,3,130,136,230,131).
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
QUIT
221 Goodbye.
----------
Connect to: (08/31/2018 1:31:36)
hostname=lab.phus.lu
username=anonymous
startdir=
lab.phus.lu=192.168.2.2
220 (vsFTPd 3.0.3)
USER anonymous
230 Login successful.
SYST
215 UNIX Type: L8
FEAT
211-Features:
 EPRT
 EPSV
 MDTM
 PASV
 REST STREAM
 SIZE
 TVFS
211 End
HELP SITE
214-The following commands are recognized.
 ABOR ACCT ALLO APPE CDUP CWD  DELE EPRT EPSV FEAT HELP LIST MDTM MKD
 MODE NLST NOOP OPTS PASS PASV PORT PWD  QUIT REIN REST RETR RMD  RNFR
 RNTO SITE SIZE SMNT STAT STOR STOU STRU SYST TYPE USER XCUP XCWD XMKD
 XPWD XRMD
214 Help OK.
OPTS UTF8 ON
200 Always in UTF8 mode.
Connect ok!
PWD
257 "/" is the current directory
读取文件夹
TYPE A
200 Switching to ASCII mode.
PASV
227 Entering Passive Mode (192,168,2,2,132,134).
Server reports local IP -> Redirect to: 192.168.2.2
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
CWD h
550 Failed to change directory.
PWD
257 "/" is the current directory
读取文件夹
PASV
227 Entering Passive Mode (192,168,2,2,67,155).
Server reports local IP -> Redirect to: 192.168.2.2
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
CDUP
250 Directory successfully changed.
PWD
257 "/" is the current directory
CDUP
250 Directory successfully changed.
PWD
257 "/" is the current directory
读取文件夹
OFFLINE6, error=0
----------
Connect to: (08/31/2018 1:35:49)
hostname=lab.phus.lu
username=anonymous
startdir=/
lab.phus.lu=192.168.2.2
220 (vsFTPd 3.0.3)
USER anonymous
230 Login successful.
SYST
215 UNIX Type: L8
FEAT
211-Features:
 EPRT
 EPSV
 MDTM
 PASV
 REST STREAM
 SIZE
 TVFS
211 End
HELP SITE
214-The following commands are recognized.
 ABOR ACCT ALLO APPE CDUP CWD  DELE EPRT EPSV FEAT HELP LIST MDTM MKD
 MODE NLST NOOP OPTS PASS PASV PORT PWD  QUIT REIN REST RETR RMD  RNFR
 RNTO SITE SIZE SMNT STAT STOR STOU STRU SYST TYPE USER XCUP XCWD XMKD
 XPWD XRMD
214 Help OK.
OPTS UTF8 ON
200 Always in UTF8 mode.
Connect ok!
CWD /
250 Directory successfully changed.
PWD
257 "/" is the current directory
读取文件夹
TYPE A
200 Switching to ASCII mode.
PASV
227 Entering Passive Mode (192,168,2,2,234,237).
Server reports local IP -> Redirect to: 192.168.2.2
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
CWD files
250 Directory successfully changed.
PWD
257 "/files" is the current directory
读取文件夹
PASV
227 Entering Passive Mode (192,168,2,2,182,135).
Server reports local IP -> Redirect to: 192.168.2.2
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
CDUP
250 Directory successfully changed.
PWD
257 "/" is the current directory
CWD H
250 Directory successfully changed.
PWD
257 "/H" is the current directory
读取文件夹
PASV
227 Entering Passive Mode (192,168,2,2,97,243).
Server reports local IP -> Redirect to: 192.168.2.2
LIST
150 Here comes the directory listing.
下载
等待服务器回应...
226 Directory send OK.
